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I. CRITERIA

In addition to applicable industry standards and specifications, the Project and associated Interconnection Customer Attachment Facilities must adhere to, and comply with, National Grid’s technical specifications (i.e., Electric System Bulletins (“ESBs”), Transmission Planning Criteria TGP28 (“TGP28”)) and its environmental and real estate guidelines and requirements provided on the National Grid Wholesale Interconnection/New York website: 

https://www.nationalgridus.com/Wholesale-Interconnections/New-York/

II. DIAGRAMS/DRAWINGS

(All applicable checkboxes must be completed.)

Conceptual Relay One Line/Single Line

Provide conceptual Relay One Line/Single Line for the Project Station (i.e., Collector Station, PSU Station). 

☐  RELAY ONE LINE/SINGLE LINE INCLUDED

[bookmark: _Hlk112161810]Preliminary Overall Project Site/Plot Plan

[bookmark: _Hlk158960146]Provide preliminary Overall Project Site/Plot Plan which must include: (i) the Generation Facility, (ii)Project Station (i.e., Collector Station, PSU Station) with coordinates for the approximate expected location of the station, (iii) proposed POI with coordinates (in decimal degrees (DD)), (iv) anticipated location(s)/route(s) of the collection system feeders, and the (v) conceptual expected route of the generator tie line(s) between the PCO and POI. 

☐  OVERALL PROJECT SITE/PLOT PLAN INCLUDED

Preliminary Overall Project Station Site/Plot Plan

Provide preliminary Project Station (i.e., Collector Station, PSU Station) Site/Plot Plan which must include: (i) the proposed layout of the Project Station in relation to the POI and transmission/distribution corridor(s), (ii) POI, (iii) coordinates for the approximate expected location of the Project Station, (iv) the anticipated location/route and length of the generator tie line between the Project Station and the PCO or POI. 

☐  PROJECT STATION SITE/PLOT PLAN INCLUDED
POI Station Site Plan

If a new POI Station (e.g., ring bus station) is required for interconnection of the project (refer to TGP28), a preliminary site plan must be provided and must include: (i) the proposed orientation of the POI Station in relation to the Project Station and POI, (ii) the transmission/distribution corridor, (iii) the POI, and (iii) coordinates (in decimal degrees (DD)) for the approximate expected location of the proposed location of the POI Station.

☐  POI STATION PRELIMINARY SITE PLAN INCLUDED
III. DATA

(All applicable checkboxes must be completed.)
[bookmark: _Toc162605458]Modeling Data Summary

All Generating Facilities shall provide a completed the Modeling Data Summary of NYISO Interconnection Projects located on the NYISO’s Interconnection Process page under Additional Request Forms & Other Forms (https://www.nyiso.com/interconnections).

☐  COMPLETED MODELING DATA SUMMARY INCLUDED
Inverter-Based Resources:

Provide cut sheets for each type of inverter.

☐  CUT SHEETS FOR EACH TYPE OF INVERTER INCLUDED
Aspen Modeling Data

All Generating Facilities shall be modeled using the appropriate type as described in ASPEN Oneliner version 15.9.

 Provide PSCAD models for each type of inverter.

☐  PSCAD MODEL FOR EACH TYPE OF INVERTER INCLUDED
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